TITLE OF THE TENDER: COI/RDRM/AO/2024/007 - SUPPLY, DELIVERY, INSTALLATION, COMMISSIONING AND AFTER-SALES SERVICE OF EQUIPMENT TO STRENGTHEN EARLY WARNING SYSTEMS IN SEYCHELLES

[bookmark: _Hlk197607601]Questions
We would be grateful if you could provide us more details for the following: 
(i)                  item 1.2 - Antenna Colinear Whip : confirm TX frequency
(ii)                item 1.21 - Yagi antenna: advise Frequency Required
(iii)               item 1.24 - Coaxial Cable Roll (m) : confirm roll length 
(iv)               confirm places of installation for appropriate costing
(v)                Please note that customer is responsible to apply appropriate licences from the Seychelles Communication Regulatory Authority to import and use these devices.
[bookmark: _Hlk197607642]Answers
(i) Item 1.2 Antenna Colinear Whip. The TX frequency is VHF 147-155 Mhz (Tx in the high end) 
(ii) Item 1.21 Yagi Antenna; Frequency required is VHF 147-155Mhz (Tx in the low end) 
(iii) Item1.24 – Coaxial Cble Roll(m) : The roll length is 30m roll
(iv) Place of installation identified as various locations of repeater sites islands of Mahe, Praslin and La Digue and base station locations in areas readily accessible by vehicular transport
(v) That is correct : The beneficiary institution at national level (DRMD) will be responsible to obtain the appropriate licences for the import and use of the devices. 

Questions
Item 1.4: ePMP 3000L 5GHz Connectorized 2x2 MIMO Access Point with GPS Sync, RoW, EU power cord            
Could you please provide the GPS coordinates of the site where the link should be installed?
Answers
I think these long range (Over 30 miles) links are now out of production.. Please can you replace with similar type probably Ubiquiti AirFibre AF-5U
I believe these Ubiquiti microwave radios should be able to acquire its own GPS coordinates as they will be used at various sites which will be decided later




Questions
Item 1.8: Heliax Connector, N-type male              
Could you confirm the model of cable required for this connector?
Answers
The cable is 1/2 inch heliax LDF4/50
Questions
Item 1.15: Double Shielded Interconnecting Cable            
Could you provide details on the type of connector and the required cable length?
Answers
The LMR400 is the cable to be used for the interconnecting cables. The coaxial connector is N Type male and the cable length for each interconnecting cable will be determined during the installation. Total length of cable is 50m and number of coaxial connectors is 40 x N-Type Male and 15 x BNC Male all for use with LMR 400
Questions
Item 1.35: Trbonet UPGRADE from Version 5.2 to 6.2 (Upgrade from 5.x to the current release version – does not extend the update subscription)              
Could you please inform us of the last updated version of Trbonet?
Answers
THE ORIGINAL VERSION of TRBOnet was 3.6 and there are not update or upgrade since 2013 and is not in use and obviously obsolete. What is required is a brand new version suitable for IPSC operation possibly 5.7 upwards with licence for 4 repeaters plus 300 radios



