Erratum:   COI/RDRM/AO/2024/007: Supply, Delivery, installation, commissioning and aftersales service of equipment to strengthen early warning systems in Seychelles 

Item 1.4: ePMP 3000L 5GHz Connectorized 2x2 MIMO Access Point with GPS Sync, RoW, EU power cord            
Could you please provide the GPS coordinates of the site where the link should be installed?
The item to be supplied should be able to acquire its own GPS coordinates such as Ubiquiti AirFibre AF-5U, as they will be used at various sites which will be decided later. 


Item 1.8: Heliax Connector, N-type male              
Could you confirm the model of cable required for this connector?
The cable is 1/2 inch heliax LDF4/50


Item 1.15: Double Shielded Interconnecting Cable            
Could you provide details on the type of connector and the required cable length?
The LMR400 is the cable to be used for the interconnecting cables. The coaxial connector is N Type male and the cable length for each interconnecting cable will be determined during the installation. Total length of cable is 50m and number of coaxial connectors is 40 x N-Type Male and 15 x BNC Male all for use with LMR 400


Item 1.35: Trbonet UPGRADE from Version 5.2 to 6.2 (Upgrade from 5.x to the current release version – does not extend the update subscription)             
Could you please inform us of the last updated version of Trbonet?
THE ORIGINAL VERSION of TRBOnet was 3.6 and there are not update or upgrade since 2013 and is not in use and obviously obsolete. What is required is a brand new version suitable for IPSC operation possibly 5.7 upwards with licence for 4 repeaters plus 300 radios
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